Gyptone Ceiling Panels - Revit Package
......................................

1. Unzip the model file and the Texture Images folder to the desired location on your local file system.

2. Open the .rvt project file in Revit 2019 and read the instruction on the start page.

3. Open the destination model which the Gyptone ceiling family should be added to.

4. Copy and past the family across to the destination project.

5. Edit the material appearance properties and assign the correct texture image to the family.

6. Layout the position and orientation of the ceiling family to suit the project needs.

7. Render and visualise the space to see which product works best.